[bookmark: _Hlk535517498]Tire Pressure Threshold
Notes
· Make sure to enable data logging and connect/backup to Google Drive
· 2018 Trucks need security bypass cable

Procedure
Key in RUN position
Open App
Connect to OBD II device
Select DODGE RAM 1500 or 2500 or 3500
                                                                         From drop down menu select BODY COMPUTER
· [bookmark: _GoBack]MY2013-17 POWERNET (2018)
· CONNECT
[image: ]             [image: ]           [image: ]
                                                                   Click on the CAR WITH THE OPEN HOOD (Active Diagnostics) 





Click SELECT PROCEDURE TO START   > Select UPDATE PRESSURE THRESHOLDS 
[image: ]            [image: ]
Select STATUS PRESSURE FRONT/REAR 
· Select desired pressure for front and rear
· START 
 [image: ]                            [image: ]



Exit BODY COMPUTER screen back to main screen
Select RADIO FREQUENCY HUB (RFH) 
Press SELECT CONTROL UNIT 
· From drop down menu select RADIO FREQUENCY HUB 
· CONNECT 
[image: ]      [image: ]
                                Click on the CAR WITH THE HOOD OPEN
Read instructions                             Click on SELECT PROCEDURE TO START > Select RF-HUB RESET/REPLACE 
[image: ]          [image: ]         
Enter 4 Digit PIN > Select START
  [image: ]

Screen should say PROCEDURE COMPLETE, shut vehicle off, open/close door and wait a minute



image6.jpeg
RLOO ATl 70% W 2:02 PM

AlfaOBD
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Connection status: Not connected

Update Pressure Thresholds -
This function will update the Tire Pressure Monitor-
ing System's Load Inflation pressures stored in the
BCM and in the TPM, if present. Use the Cold Tire
Inflation Pressure for the front and rear tires listed

on the Tire and Loading Information label located
on the inside driver's door or driver's door jam.

Status Pressure Front: -

Status Pressure Rear: -

START

STOP
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Connect requested to: Body computer

CONNECT

Automatic reconnect

Connection status: Not connected
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Connection status: Not connected

Select procedure to start v

WARNING:

- For the active diagnostics turn the engine off
leaving key in MAR. For the models equipped
with Stop&Start system the procedures must be
run with the engine actually stopped (Stop&Start
function off).For certain procedures engine must
be started, read on-screen instructions.

- Check for errors stored and fix them before
running diagnostics otherwise it might be not
reliable or not possible.

The list of procedures is updated when connection
to particular control unit is established, so the list
might be incomplete in idle.

Some active diagnostic procedures might not be
supported depending on the vehicle version!

START

STOP
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View Ignition (IGNM/KIN) Part Information
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Active Diagnostics
Connection status: Not connected

RF-HUB Reset/Replace -

Use this function when the RF-HUB has been
replaced or when the Body computer configuration
has been changed to make the RF HUB to learn
the new configuration. Ignition FOBIK(s) must

be programmed before running this function.
Programmed FOBIK(s) must be inside the vehicle.
Set the Start switch to the RUN position. Enter PIN
into the box below and press 'Start'.

Enter PIN (4 digits):

START

STOP
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Connect requested to: Body computer

CONNECT
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Connection status: Not connected

Select procedure to start .

WARNING:

- For the active diagnostics turn the engine off
leaving key in MAR. For the models equipped
with Stop&Start system the procedures must be
run with the engine actually stopped (Stop&Start
function off).For certain procedures engine must
be started, read on-screen instructions.

- Check for errors stored and fix them before
running diagnostics otherwise it might be not
reliable or not possible.

The list of procedures is updated when connection
to particular control unit is established, so the list
might be incomplete in idle.

Some active diagnostic procedures might not be
supported depending on the vehicle version!
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